%% Based on a TeXnicCenter-Template, which was
%% created by Christoph Börensen
%% and slightly modified by Tino Weinkauf.
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%

\documentclass[a4paper,11pt]{scrartcl} %This is a special class provided by the KOMA script, which does a lot of adjustments to adapt the standard LaTeX classes to european habits, change to [a4paper,12pt,twoside] for doublesided layout scrartcl


%########################### Preferences #################################


% ******** vmargin settings *********
\usepackage{vmargin} %This give you full control over the used page arae, it maybe not the idea od Latex to do so, but I wanted to reduce to amount of white space on the page
\setpapersize{A4}
\setmargins{1.5cm}%			left edge
					 {1.5cm}%     top edge
           {18cm}%			text width
           {23.42cm}%   text hight
           {14pt}%			header hight
           {1cm}%   	  header distance
           {0pt}%				footer hight
           {2cm}%    	  footer distance         

% ********* Font definiton ************
\usepackage{t1enc} % as usual
\usepackage[latin1]{inputenc} % as usual
\usepackage{times}	
\usepackage{tabularx}	
\usepackage{sectsty}
\usepackage{textcomp}

\usepackage{titlesec}

% ********* TEXTBLOCK ***********
\usepackage[absolute]{textpos} 
%\TPshowboxestrue % commenter une fois fini
\TPshowboxesfalse % décommenter pour faire disparaitre les boites
\textblockorigin{10mm}{10mm} % origine des positions

\usepackage[T1]{fontenc}
\usepackage[francais]{babel}
\usepackage{lastpage}
%\usepackage{mathptmx}  	%mathematical fonts for use with times, I encountered some problems using this package togather with pdftex, which I was not able to resolve

% ********* Graphics definition *******
\usepackage[pdftex]{graphicx} % required to import graphic files
\usepackage{color} %allows to mark some entries in the tables with color
\usepackage{colortbl}
\usepackage{wrapfig}
\usepackage{eso-pic} % these two are required to add the little picture on top of every page
\usepackage{everyshi} % these two are required to add the little picture on top of every page
\renewcommand{\floatpagefraction}{0.7} %default:0.5 allows two big pictures on one page

%********** Enybeling Hyperlinks *******
\usepackage[pdfborder=000,pdftex=true]{hyperref}% this enables jumping from a reference and table of content in the pdf file to its target

% ********* Table layout **************
\usepackage{booktabs}	  	%design of table, has an excellent documentation
%\usepackage{lscape}			%use this if you want to rotate the table together with the lines around the table

% ********* Caption Layout ************
\usepackage{ccaption} % allows special formating of the captions
\captionnamefont{\bf\footnotesize\sffamily} % defines the font of the caption name (e.g. Figure: or Table:)
\captiontitlefont{\footnotesize\sffamily} % defines the font of the caption text (same as above, but not bold)
\setlength{\abovecaptionskip}{0mm} %lowers the distace of captions to the figure


% ********* Header and Footer **********
% This is something to play with forever. I use here the advanced settings of the KOMA script

\usepackage{scrpage2} %header and footer using the options for the KOMA script
\renewcommand{\headfont}{\footnotesize\sffamily} % font for the header
\renewcommand{\pnumfont}{\footnotesize\sffamily} % font for the pagenumbers

%the following lines define the pagestyle for the main document
\defpagestyle{cb}{%
(\textwidth,0pt)% sets the border line above the header
{\pagemark\hfill\headmark\hfill}% doublesided, left page
{\hfill\headmark\hfill\pagemark}% doublesided, right page
{\hfill\headmark\hfill\pagemark}%  onesided
(\textwidth,1pt)}% sets the border line below the header
%
{(\textwidth,1pt)% sets the border line above the footer
%{{\thepage\ / \pageref{LastPage}}\hfill{Tobeca SARL – Guide de montage de la Tobeca®}}% doublesided, left page
{Tobeca SARL - www.tobeca.fr\hfill{\it Tobeca\textregistered~ assembly guide}}% doublesided, left page
{Tobeca SARL - www.tobeca.fr\hfill{\it Tobeca\textregistered~ assembly guide}}% doublesided, right page
{Tobeca SARL - www.tobeca.fr\hfill{\it Tobeca\textregistered~ assembly guide}} % one sided printing
(\textwidth,0pt)% sets the border line below the footer
}

%this defines the page style for the first pages: all empty
\renewpagestyle{plain}%
	{(\textwidth,0pt)%
		{\hfill}{\hfill}{\hfill}%
	(\textwidth,0pt)}%
	{(\textwidth,0pt)%	
		{\hfill}{\hfill}{\hfill}%
	(\textwidth,0pt)}

%********** Footnotes **********
\renewcommand{\footnoterule}{\rule{5cm}{0.2mm} \vspace{0.3cm}} %increases the distance of footnotes from the text
\deffootnote[1em]{1em}{1em}{\textsuperscript{\normalfont\thefootnotemark}} %some moe formattion on footnotes

%********** Logo Tobeca SARL **********
\newcommand{\logotobeca}{ %pour afficher le logo Tobeca SARL sur toutes les pages
\begin{textblock*}{3cm}[0,0](25mm,20mm) 
\includegraphics[scale=0.04]{images/logo_tobeca.jpg} 
\end{textblock*}} 

%configuration des sections
\titleformat*{\section}{\vspace*{2cm}\Huge\bf\sf\filcenter}

%################ End Preferences, Begin Document #####################

\pagestyle{plain} % on headers or footers on the first page
%\allsectionsfont{\centering}

\begin{document}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%Page de titre
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\begin{center}
\logotobeca
\vspace{2cm}
{\Huge\bf\sf Tobeca\textregistered~ assembly guide}
\vspace{.5cm}

{\bf\sf\it Open source foldable 3D printer}
\vspace{2cm}

{\Large\bf\sf Tobeca SARL - Adrien Grelet}
\vspace{0.5cm}

\begin{figure}[th]
    \centering
		\includegraphics[width=0.9\textwidth]{images/DSC02489.JPG}
\end{figure}

\end{center}

\pagestyle{cb} % now we want to have headers and footers

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%Note de versions
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\section{Changelog}
\vspace{1cm}

\subsection{v1.0 of 25/01/2014}
First final version of this guide, directly translated from the french v1.0.\\

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%Sommaire
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\tableofcontents

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%Introduction
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\section{Introduction}
\newpage

The assembly of a Tobeca\textregistered~ will allow you to understand from A to Z how your Tobeca\textregistered~ works. Depending on your skills, the assembly will take beetween 15 to 30 hours to be finished.\\

N'oubliez pas de prendre toutes les précautions nécessaires pour éviter tout accident pendant l'assemblage, notamment lors des soudures avec un fer à souder.\\

En cas de doute, n'hésitez pas à poser vos questions sur le forum ou sur la communauté Google+.\\

L'assemblage d'un kit Tobeca\textregistered~ vous demandera l'outillage suivant :\\
\begin{itemize}
\item Marteau
\item Pince plate
\item Pince coupante
\item Fer à souder et étain
\item Ciseaux
\item Cutter
\item TourneScrews cruciforme Pozidrive PZ1
\item TourneScrews plat de précision (pour ajustement puissance moteurs)
\item Papier de verre
\item Clé plate pour écrous M3 (5,5mm)
\item Clés BTR (à empreinte hexagonale)
\item Sèche cheveux ou décapeur thermique (pour les gaînes thermorétractables)
\item Superglue ou colle époxy (utilisé en très petite Quantity)\\
\end{itemize}

Les printed parts fournies dans un kit sont brutes d'impression. Un montage en direct n'a pas d'influence sur les performances mécaniques. Cependant, pour améliorer l'esthétique de la machine, un léger grattage/ponçage peut être réalisé avec un cutter ou un papier de verre fin.

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%Section PRE : Préparation des pièces
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\section{PRE - Parts preparation}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%PRE-0010
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
PRE-0010 & Mise en place des écrous dans les printed parts & Montage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{ReScrewsion} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Standard M3 nuts & 57 & \\
\hline
Nylstop M3 nuts & 9 & ont une petite collerette en nylon\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/PRE/DSC02318.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter les écrous dans les printed parts. Les points rouges sont pour les standard M3 nuts et les points verts pour les écrous M3 Nylstop. Les écrous Nylstop sont à monter avec le joint vers le haut. & Pour les écrous à monter horizontalement, les Screwsser sur une Screws pour les monter en frappant la Screws avec un marteau. Pour les écrous à monter verticalement, utiliser un marteau pour les enfoncer puis une Screws pour les faire descendre.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%PRE-0020
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
PRE-0020 & Préparation des molettes de serrage & Montage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
MOLETTE\_GRANDE & 4 & printed parts, assembled with standard M3 nuts\\
\hline
Screws M3x30mm & 4 & \\
\hline
Standard M3 nuts & 8 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/PRE/DSC02319.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Screw the screws M3x30mm on the MOLETTE_GRANDE, tighting with the already in place nut. Then add 2 standards M3 nuts onto. Tight well this assembly, you can add a drop of superglue. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%PRE-0030
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
PRE-0030 & Préparation de la molette de réglage de l'offset Z & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
MOLETTE\_GRANDE & 1 & printed part, with standard M3 nut\\
\hline
Screws M3x40mm & 1 & \\
\hline
Ecrou M3 standard & 1 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/PRE/DSC02320.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Screwsser la Screws M3x40mm sur la molette, en serrant avec l'écrou déjà en place. Ajouter ensuite un standard M3 nut par dessus le premier écrou. Bien serrer voire ajouter un point de superglue. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%PRE-0040
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
PRE-0040 & Préparation des molettes de serrage pour l'extrudeur & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
MOLETTE\_PETITE & 2 & printed parts, montées avec les standard M3 nuts\\
\hline
Screws M3x60mm & 2 & \\
\hline
Standard M3 nuts & 2 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/PRE/DSC02321.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Screwsser les Screws M3x60mm sur les molettes, en serrant avec les écrous déjà en place. Ajouter ensuite un standard M3 nuts par dessus le premier écrou. Bien serrer voire ajouter un point de superglue. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%PRE-0050
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
PRE-0050 & Préparation des TOP\_Z & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
TOP\_Z & 2 & printed parts\\
\hline
Screws M3x10mm & 4 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/PRE/DSC02322.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Screwsser les Screws M3x10mm sur les TOP\_Z, sans serrer. Nettoyer ensuite avec un cutter les pourtours des trous (indiqués par les flèches rouges). & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%PRE-0060
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
PRE-0060 & Préparation des contacts de fin de course & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Contacts de fin de course & 3 & \\
\hline
Paire RJ45 900mm & 1 & \\
\hline
Paire RJ45 500mm & 2 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/PRE/DSC02416.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Souder les paires RJ45 aux contacts de fin de course. & Ne pas souder le contact du milieu.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%PRE-0070
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
PRE-0070 & Préparation des contacts de fin de course & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Contacts Molex & 6 & \\
\hline
Connecteur Molex 3 pôles & 3 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/PRE/DSC02418.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/PRE/DSC02421.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Souder à l'extrémité des paires RJ45 des contacts Molex puis les insérer dans les connecteurs Molex sur les 2 pôles extérieurs. & Pour souder les contacts Molex, mettre un point de soudure puis utiliser une pince pour pincer un peu les bords. Le contact doit se bloquer avec sa petite patte anti retour.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%POR-0080
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
PRE-0080 & Préparation des accouplements & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
COUPLAGE\_Z & 2 & printed parts \\
\hline
Screws M3x10mm & 4 & \\
\hline
Standard M3 nuts & 4 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/POR/DSC02396.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter les écrous et les Screws M3x10mm dans les COUPLAGE\_Z. Ne pas serrer pour l'instant. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%Section MAL : Finition de la mallette
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\section{MAL - Finition de la mallette}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%MAL-0010
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
MAL-0010 & Fixation des fermetures grenouilles dans le châssis & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 12/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Fermetures grenouilles & 4 & partie basse\\
\hline
Screws M3x16mm à tête fraisée & 12 & \\
\hline
Rondelles M3 larges & 12 & \\
\hline
Ecrous M3  standards & 12 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/MAL/DSC01830.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter les parties basses des fermetures grenouilles dans le châssis. Ne pas oublier les rondelles M3 larges avant de mettre l'écrou. & Faire affleurer les fermetures sur le bord du bois.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%MAL-0020
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
MAL-0020 & Fixation des fermetures grenouilles dans le capot & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 12/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Fermetures grenouilles & 4 & partie haute\\
\hline
Screws M3x16mm à tête fraisée & 12 & \\
\hline
Rondelles M3 larges & 12 & \\
\hline
Standard M3 nuts & 12 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/MAL/DSC01835.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter les parties hautes des fermetures grenouilles dans le capot. & Faire affleurer les fermetures sur le bord du bois.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%MAL-0030
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
MAL-0030 & Fixation de la poignée sur le capot & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 12/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Poignée & 1 & prémontée avec la Screwsserie\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/MAL/DSC01834.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter la poignée dans les trous prévus dans le capot. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%MAL-0040
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
MAL-0040 & Fixation de l'étiquette sur le capot & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 12/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
ETIQUETTE & 1 & printed part\\
\hline
Screws M3x16mm à tête fraisée & 2 & \\
\hline
Rondelles M3 larges & 2 & \\
\hline
Rondelles M3 standards & 2 & \\
\hline
Standard M3 nuts & 2 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/MAL/DSC01833.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter L'étiquette sur le capot, les rondelles M3 standards sur l'ETIQUETTE et les rondelles M3 larges à l'intérieur de la mallette.  & Attention au sens de Assembly (voir photo).\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%Section CHA : Assembly des printed parts dans le châssis
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\section{CHA - Assembly des printed parts dans le châssis}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CHA-0010
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CHA-0010 & Fixation des RANGEMENT\_PORTIQUE & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
RANGEMENT\_PORTIQUE & 4 & printed parts\\
\hline
Screws M3x16mm à tête fraisée & 8 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CHA/DSC02323.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CHA/DSC02324.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter les RANGEMENT\_PORTIQUE dans le châssis avec les Screws M3x16mm à tête fraisée, dans les trous fraisés correspondant.  & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CHA-0020
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CHA-0020 & Fixation du ventilateur dans SANGUINOLOLU\_CASE & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
SANGUINOLOLU\_CASE & 1 & printed part\\
\hline
Ventilateur 40mm & 1 & \\
\hline
Screws M3x20mm à tête fraisée & 4 & \\
\hline
Rondelles M3 standards & 4 & \\
\hline
Standard M3 nuts & 4 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CHA/DSC02353.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CHA/DSC02354.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter le ventilateur à l'extérieur du boitier, en passant les fils dans le trou pour pouvoir le brancher sur la carte électronique. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CHA-0030
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CHA-0030 & Fixation de la pièce SANGUINOLOLU\_CASE dans le châssis & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Screws M3x20mm  & 4 & \\
\hline
Rondelles M3 larges & 4 & \\
\hline
Standard M3 nuts & 4 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/CHA/DSC02355.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter le boitier dans le châssis avec les Screws M3x20mm, en mettant les rondelles larges à l'extérieur. & Il n'y a pas besoin de rondelles à l'intérieur du boitier car il y a des empreintes pour les écrous prévues dans le boitier.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CHA-0040
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CHA-0040 & Fixation des BASE\_Z dans le châssis & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
BASE\_Z & 2 & printed parts\\
\hline
Screws M3x20mm  & 4 & \\
\hline
Rondelles M3 larges & 4 & \\
\hline
Rondelles M3 standards & 4 & \\
\hline
Standard M3 nuts & 4 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CHA/DSC02357.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CHA/DSC02356.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Screwsser les deux BASE\_Z en s'assurant qu'un tube de 12mm peut passer sans trop forcer dans les trous (ébavurer si nécessaire) avec les Screws M3x20mm. Les rondelles M3 larges sont à l'extérieur du châssis et les rondelles M3 standards sont à l'intérieur. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%Section ELE : Assembly de l'électronique
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\section{ELE - Assembly de l'électronique}

\newpage
La carte de la Tobeca\textregistered~ possède déjà le FTDI soudé. Il ne reste donc plus qu'à souder les composants “classiques”.\\

Si vous avez reçu une carte déjà entièrement soudée, il faut tout de même souder les contacts 12v sur les bords de la carte pour les ventilateurs et la LED. Voir l'étape ELE-0120.

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%ELE-0010
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
ELE-0010 & Soudure de résistances & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 07/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Nom} & \textbf{Description} & \textbf{Code couleur, notes}\\
\hline
R1 & Résistance 1 kohms & marron, noir, rouge\\
\hline
R2 & Résistance 100 kohms & marron, noir, jaune\\
\hline
R3 & Résistance 100 kohms & marron, noir, jaune\\
\hline
R4 & Résistance 100 kohms & marron, noir, jaune\\
\hline
R5 & Résistance 100 kohms & marron, noir, jaune\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/ELE/sanguino1.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|c|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Souder les 5 premières résistances sur la carte. & Attention car l'espace entre les trous n'est pas grand. Cela signifie qui faut bien plier les pattes des résistances à raz.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%ELE-0020
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
ELE-0020 & Soudure de résistances & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 07/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Nom} & \textbf{Description} & \textbf{Code couleur, notes}\\
\hline
R6 & Résistance 10 kohms & marron, noir, orange\\
\hline
R7 & Résistance 100 kohms & marron, noir, jaune\\
\hline
R8 & Résistance 100 kohms & marron, noir, jaune\\
\hline
R9 & Résistance 4.7 kohms & jaune, violet, rouge\\
\hline
R10 & Résistance 4.7 kohms & jaune, violet, rouge\\
\hline
R11 & Résistance 10 kohms & marron, noir, orange\\
\hline
R12 & Résistance 100 kohms & marron, noir, jaune\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/ELE/sanguino2.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Souder les résistances sur la carte. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%ELE-0030
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
ELE-0030 & Soudure de condensateurs & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 08/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Nom} & \textbf{Description} & \textbf{Code couleur, notes}\\
\hline
C6 & Condensateur $0.1µF$ & \\
\hline
C7 & Condensateur $0.1µF$ & \\
\hline
C8 & Condensateur $0.1µF$ & \\
\hline
C11 & Condensateur $0.1µF$ & \\
\hline
C13 & Condensateur $0.1µF$ & \\
\hline
C14 & Condensateur $0.1µF$ & \\
\hline
C15 & Condensateur $0.1µF$ & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/ELE/sanguino3.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|c|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Souder les condensateurs sur la carte. & Ces condensateurs n'ont pas de polarités. Ils peuvent donc être montés dans n'importe quel sens.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%ELE-0040
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
ELE-0040 & Soudure de composants & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 08/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Nom} & \textbf{Description} & \textbf{Code couleur, notes}\\
\hline
S1 & Bouton Reset & \\
\hline
LED & Diode LED rouge & \\
\hline
Y1 & résonateur 16MHz 22pF & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/ELE/sanguino4.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|c|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Souder les composants sur la carte. & Attention au sens de Assembly de la LED (le méplat est symbolisé sur la carte). Concernant le bouton reset, mettre les sorties des pattes à gauche et à droite). Le résonateur peut être monté dans n'importe quel sens.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%ELE-0050
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
ELE-0050 & Soudure de condensateurs & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 08/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Nom} & \textbf{Description} & \textbf{Code couleur, notes}\\
\hline
C1 & Condensateur $100µF$ & \\
\hline
C2 & Condensateur $100µF$ & \\
\hline
C3 & Condensateur $100µF$ & \\
\hline
C4 & Condensateur $100µF$ & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/ELE/sanguino5.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|c|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Souder les condensateurs sur la carte. & Attention à la polarité des condensateurs, le moins est indiqué par la bande noire sur le composant et est marqué sur la carte.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%ELE-0060
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
ELE-0060 & Soudure de condensateurs & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 08/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Nom} & \textbf{Description} & \textbf{Code couleur, notes}\\
\hline
C16 & Condensateur $4.7µF$ & \\
\hline
C9 & Condensateur $10µF$ & \\
\hline
C10 & Condensateur $10µF$ & \\
\hline
C5 & Condensateur $0.33µF$ & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/ELE/sanguino6.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|c|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Souder les condensateurs sur la carte. & Attention à la polarité pour C16, C9 et C10.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%ELE-0070
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
ELE-0070 & Soudure de jumpers et barrettes & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 08/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Nom} & \textbf{Description} & \textbf{Quantity}\\
\hline
Barrette 32 pattes &  & 2\\
\hline
Picots 6 pattes &  & 4\\
\hline
Jumpers 2 points &  & 12\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/ELE/sanguino7.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Souder tout d'abord les picots 6 pattes à l'emplacement où seront les jumpers puis les barrettes à 32 pattes. Mettre ensuite 3 jumpers par picots 6 pattes, permettant d'avoir un micropas des moteurs de 1\textbackslash{}16. & Pour mettre en place les picots, l'astuce consiste à mettre au préalable un point d'étain dans un trou et mettre ensuite le picot en faisant fondre le point. Il sera ainsi déjà bloqué et la soudure des autres pattes sera plus facile.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%ELE-0080
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
ELE-0080 & Soudure jumper et microprocesseur & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 08/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Nom} & \textbf{Description} & \textbf{Code couleur, notes}\\
\hline
Picot 2 pattes &  & \\
\hline
Jumper 2 points &  & \\
\hline
Support microprocesseur &  & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/ELE/sanguino8.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter le jumper d'autoreset puis le support pour le microprocesseur. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%ELE-0090
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
ELE-0090 & Soudure de composants & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 08/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Nom} & \textbf{Description} & \textbf{Code couleur, notes}\\
\hline
Bornier 2 pôles &  & \\
\hline
Prise USB &  & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/ELE/sanguino9.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|c|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Ajouter le bornier vert pour l'alimentation et la prise USB. & Bien souder les grosses pattes de la prise USB pour quelle soit bien fixée.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%ELE-0100
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
ELE-0100 & Soudure de composants & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 08/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Nom} & \textbf{Description} & \textbf{Code couleur, notes}\\
\hline
LM7805 & Régulateur de tension & \\
\hline
Q1 & Mosfet IRLB743 & \\
\hline
Q2 & Mosfet IRLB743 & \\
\hline
C12 & Condensateur $1000µF$ & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/ELE/sanguino10.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|c|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter les trois composants sur la carte. & Attention au sens de Assembly, toujours les parties métalliques vers l'extérieur. Attention aussi à la polarité de C12.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%ELE-0110
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
ELE-0110 & Soudure de connecteurs Molex & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 08/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Nom} & \textbf{Description} & \textbf{Code couleurs, notes}\\
\hline
Connecteurs Molex mâle 4 pattes &  & \\
\hline
Connecteurs Molex mâle 3 pattes &  & \\
\hline
Connecteurs Molex mâle 2 pattes &  & \\
\hline
Borniers 4 pôles &  & en fonction des kits\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/ELE/sanguino11.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Souder ensuite les connecteurs Molex pour brancher les moteurs, thermistances, résistances et contacts de fin de course. & En fonction des kits, les connecteurs pour les résistances de chauffe plateau et tête d'impression peuvent avoir été remplacés par des borniers à Screws (les deux connecteurs de gauche).
Aussi, les connecteurs blancs peuvent être verticaux.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%ELE-0120
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
ELE-0120 & Soudure de picots & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 08/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Nom} & \textbf{Description} & \textbf{Code couleurs, notes}\\
\hline
Picots 2 pattes &  & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/ELE/sanguino12.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Souder ensuite 4 connecteurs sur les 4 sorties 12V. Ils permettront de brancher l'éclairage et la ventilation. & Dans la pratique, trois sorties 12V pourront être utilisées mais cela permet plus de souplesse lors du câblage.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%ELE-0130
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
ELE-0130 & Assembly des drivers de moteurs & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 08/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Nom} & \textbf{Description} & \textbf{Quantity}\\
\hline
Drivers de moteurs &  & 4\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/ELE/sanguino14.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|c|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter les drivers de moteurs. & Attention car le sens de branchement est très important. Les monter comme indiqué sur la photo.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%ELE-0140
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
ELE-0140 & Assembly des radiateurs sur les drivers & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 08/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Nom} & \textbf{Description} & \textbf{Quantity}\\
\hline
Radiateurs de puces &  & 4\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/ELE/sanguino15.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Coller enfin les radiateurs sur les puces avec le double face fourni. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%ELE-0150
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
ELE-0150 & Installation du microprocesseur & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 08/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Nom} & \textbf{Description} & \textbf{Code couleurs, notes}\\
\hline
Microprocesseur ATMega 1284p&  & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/ELE/sanguino16.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Pour finir, installer le microprocesseur sur la carte, le demi cercle à droite. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%Section FIX : Fixation électronique et alimentation + raccordement électrique
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\section{FIX - Fixation électronique et alimentation + raccordement électrique}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%FIX-0010
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
FIX-0010 & Fixation de l'alimentation dans le châssis & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Alimentation électrique & 1 & \\
\hline
Screws M3x20mm & 4 & \\
\hline
Rondelles M3 larges & 4 & \\
\hline
Standard M3 nuts & 4 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/FIX/DSC02358.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Screwsser l'alimentation électrique dans le châssis avec les Screws M3x20mm. Les rondelles larges vont du côté extérieur. & Il n'y a pas de rondelles à mettre à l'intérieur.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%FIX-0020
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
FIX-0020 & Câblage du connecteur IEC & Câblage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Connecteur IEC & 1 & \\
\hline
Câble $0.75mm²$ & 1 & \\
\hline
Câble $1.5mm²$ de terre & 1 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/FIX/DSC02359.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Souder les fils comme indiqués sur l'image. Les départs pour se raccorder à l'alimentation doivent faire environ 10cm. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%FIX-0030
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
FIX-0030 & Fixation du connecteur IEC dans la plaque arrière & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Connecteur IEC câblé & 1 & \\
\hline
PLAQUE\_ARRIERE & 1 & printed part\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/FIX/DSC02360.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Clipser le connecteur IEC dans la PLAQUE\_ARRIERE. & Il est absolument nécessaire que le connecteur soit bien maintenu sur la plaque, qu'il ne puisse pas se défaire en débranchant la prise par exemple.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%FIX-0040
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
FIX-0040 & Câblage à l'alimentation & Câblage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Câble double $0.75mm²$ & 300mm & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/FIX/DSC02361.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Brancher les câbles sur le bornier comme indiqué sur la photo. Le câble double de 30cm servira à alimenter la carte électronique. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%FIX-0050
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
FIX-0050 & Fixation de la plaque arrière & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
PLAQUE\_ARRIERE complète & 1 & \\
\hline
Screws M3x20mm & 4 & \\
\hline
Rondelles M3 standards & 8 & \\
\hline
Standard M3 nuts & 4 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/FIX/DSC02362.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter la plaque arrière dans le châssis avec les Screws M3x20mm. Il faut mettre des rondelles à l'intérieur et à l'extérieur. & Bien serrer la plaque arrière, il en va de la sécurité électrique de l'imprimante !\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%FIX-0060
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
FIX-0060 & Fixation de la carte électronique & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Carte électronique & 1 & \\
\hline
Standard M3 nuts & 2 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/FIX/DSC02363.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter la carte électronique en mettant deux écrous M3 en diagonale.& Pas besoin de serrer pour le moment, il faudra le faire une fois tout le câblage réalisé.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%Section HBE : Assembly du plateau chauffant
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\section{HBE - Assembly du plateau chauffant}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%HBE-0010
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
HBE-0010 & Schéma de câblage du plateau & Schéma\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 12/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/HBE/schema_cablage.jpg}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
On remarque bien les 3 groupes de 3 résistances en parallèle, permettant d'obtenir \textbf{21.82W} sous 12V par groupe soit au total : \[21.82 \times 3 = 65.46W\] & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%HBE-0020
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
HBE-0020 & Schéma des résistances du plateau & Schéma\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 12/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/HBE/placement_resistances.jpg}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Pour la ligne centrale, les mesures de placement des résistances hautes et basses ont pour référence la patte de connexion des résistances et non pas le corps. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%HBE-0030
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
HBE-0030 & Collage des résistances & Assembly \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 12/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Résistances chauffantes & 9 & \\
\hline
Adhésif thermique & 1.5 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/HBE/DSC02524.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Coller les résistances avec le double face thermique fourni, les trous fraisés à l'opposé. & Attention car il y a tout juste la bonne Quantity d'adhésif pour les 9 résistances.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%HBE-0040
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
HBE-0040 & Câblage de la thermistance & Câblage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 12/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Thermistance & 1 & \\
\hline
Paire RJ45 500mm & 1 & \\
\hline
Contacts Molex & 2 & \\
\hline
Connecteur Molex 2 pôles & 1 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/HBE/DSC02525.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/HBE/DSC02526.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Souder les fils à la thermistance et monter un connecteur Molex deux pôles à l'extrémité. Couper ensuite l'excédent des pattes de la thermistance. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%HBE-0050
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
HBE-0050 & Collage de la thermistance & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 12/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Adhésif Kapton &  & ou adhésif standard si non disponible \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/HBE/DSC02527.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/HBE/DSC02528.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Coller une première bande d'adhésif sur le plateau pour l'isoler électriquement et coller ensuite la thermistance avec une autre bande. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%HBE-0060
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
HBE-0060 & Câblage du plateau & Câblage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 12/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Câble double $0.75mm²$ & 1 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/HBE/DSC02529.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Câbler les résistances du plateau conformément à HBE-0010. Monter ensuite un câble double de 50cm qui sera raccordé à la carte électronique. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%HBE-0070
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
HBE-0070 & Screws de coin du plateau & Câblage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 12/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Screws M3x40mm à tête fraisée & 4 & \\
\hline
Rondelles M3 standards & 16 & \\
\hline
Standard M3 nuts & 4 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/HBE/DSC02530.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/HBE/DSC02531.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter les Screws M3x40mm à tête fraisée avec 4 rondelles avant l'écrou. Bien serrer. & Eventuellement mettre un point de colle pour bloquer les écrous.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%HBE-0080
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
HBE-0080 & Contact de fin de course Y et rassemblement des câbles & Câblage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 12/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
CLIP\_PLATEAU & 2 & printed parts\\
\hline
Contact de fin de course & 1 & avec fils de 500mm \\
\hline
Spirale de câble & 500mm & \\
\hline
Screws M3x16mm à tête fraisée & 4 & \\
\hline
Rondelles M3 standards & 4 & \\
\hline
Standard M3 nuts & 4 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/HBE/DSC02532.JPG}
\vspace{0.5cm}

\newpage

%Image
\includegraphics[width=\textwidth]{images/HBE/DSC02533.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Ajouter le contact de fin de course pour l'axe Y en le laissant déborder un peu vers la droite en longueur. Ajouter la gaîne spirale puis monter les CLIP\_PLATEAU avec les Screws M3x16mm à tête fraisée. Bien serrer. & Attention à ne pas pincer les câbles avec les CLIP\_PLATEAU car cela pourrait les sectionner à la longue.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%Section AXY : Assembly de l'axe Y
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\section{AXY - Assembly de l'axe Y}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%AXY-0010
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
AXY-0010 & Suppression des Screws du moteur pour l'axe Y & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Moteur NEMA17 & 1 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/AXY/DSC02364.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Enlever les 4 Screws du moteur NEMA17  & Utiliser un tourneScrews adapté pour ne pas abîmer les têtes de Screws.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%AXY-0020
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
AXY-0020 & Fixation du moteur pour l'axe Y dans le châssis & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Moteur NEMA17 & 1 & avec les Screws précédemment enlevées\\
\hline
Screws M3x60mm & 4 & \\
\hline
Rondelles M3 larges & 4 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/AXY/DSC02365.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
ReScrewsser le moteur NEMA17 à travers le bois du châssis avec les Screws M3x60mm et les rondelles larges à l'extérieur. & Attention à l'orientation du connecteur du moteur (voir photo).\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%AXY-0030
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
AXY-0030 & Fixation du RETOUR\_Y\_BASE & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
RETOUR\_Y\_BASE & 1 & printed part\\
\hline
Roulement 608ZZ & 1 & \\
\hline
Screws M3x20mm & 2 & \\
\hline
Rondelles M3 standards & 2 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/AXY/DSC02366.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Screwsser le RETOUR\_Y\_BASE au fond du châssis avec les Screws M3x20mm et leur rondelle à l'extérieur. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%AXY-0040
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
AXY-0040 & Fixation des CHARIOT\_Y\_LM8UU sur le support plateau & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
CHARIOT\_Y\_LM8UU & 3 & printed parts\\
\hline
Screws M3x16mm à tête fraisée & 3 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/AXY/DSC02367.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/AXY/DSC02368.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Screwsser les CHARIOT\_Y\_LM8UU sur le support plateau avec les Screws M3x16mm à tête fraisée. & Attention au sens de Assembly (voir photos). Serrer les Screws pour que les têtes fraisées rentrent dans le bois jusqu'à l'affleurer. \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%AXY-0050
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
AXY-0050 & Fixation des douilles linéaires sur le support plateau & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Douilles à billes LM8UU & 3 & \\
\hline
Colliers nylon 200mm & 6 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/AXY/DSC02369.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Fixer les douilles à billes avec les colliers nylon de 200mm. & Vérifier que les CHARIOT\_Y\_LM8UU sont propres et sans bavures avant le Assembly. Si nécessaire, poncer l'intérieur avec du papier de verre. Attention au sens de Assembly des colliers (voir photo). \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%AXY-0060
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
AXY-0060 & Fixation des Screws pour la courroie Y & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Screws M3x20mm à tête fraisée & 2 & \\
\hline
Rondelles M3 standards & 2 & \\
\hline
Standard M3 nuts & 2 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/AXY/DSC02370.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Mettre en place les Screws M3x20mm à tête fraisée dans les trous centraux avec les rondelles et les écrous. & La partie filetée des Screws est à l'opposé des douilles à billes. Serrer les Screws pour que les têtes fraisées rentrent dans le bois jusqu'à l'affleurer. \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%AXY-0070
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
AXY-0070 & Mise en place des arbres de guidage & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Arbres de guidage 8x420mm & 2 & \\
\hline
SUPPORT\_AXE\_Y\_8MM & 4 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/AXY/DSC02371.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/AXY/DSC02372.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Mettre 2 SUPPORT\_AXE\_Y\_8MM à l'extrémité des arbres de guidage et les enfiler dans les douilles du support plateau. Remettre ensuite les 2 autres SUPPORT\_AXE\_Y\_8MM. & Pour un Screwssage plus simple de l'ensemble ensuite, il est préférable d'aligner les SUPPORT\_AXE\_Y\_8MM. \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%AXY-0080
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
AXY-0080 & Fixation de la poulie sur le moteur de l'axe Y & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Poulie aluminium & 1 & \\
\hline
Screws M3x8mm & 1 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/AXY/DSC02374.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter la poulie sur l'arbre du moteur de l'axe Y. Commencer à serrer la Screws M8 sur le méplat du moteur. & Ne pas serrer à fond, pour permettre un réglage de la hauteur avec la courroie. \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%AXY-0090
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
AXY-0090 & Mise en place de la courroie & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Courroie d'entraînement 840mm & 1 & \\
\hline
Collier nylon 200mm & 1 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/AXY/DSC02380.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Faire une boucle sur la courroie avec le collier nylon. Passer la boucle sur la Screws à tête fraisée M3x20mm du support plateau (côté RETOUR\_Y\_BASE). & Finir de serrer le collier autour de la Screws pour qu'il n'y ai pas de jeu au niveau de la boucle. Attention au sens du collier nylon (voir photo). \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%AXY-0100
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
AXY-0100 & Fermeture du groupe RETOUR\_Y & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
RETOUR\_Y\_TOP & 1 & printed part\\
\hline
Screws agglo 4x20mm à tête fraisée & 2 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/AXY/DSC02376.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/AXY/DSC02377.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Faire un demi tour à la courroie pour que le plat soit en contact avec le roulement 608ZZ. Screwsser ensuite le RETOUR\_Y\_TOP sur le RETOUR\_Y\_BASE avec les Screws agglo à tête fraisée. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%AXY-0110
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
AXY-0110 & Assembly de la courroie de l'axe Y & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Collier nylon 200mm & 1 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/AXY/DSC02381.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Faire une boucle très serrée à l'autre extrémité de la courroie. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%AXY-0120
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
AXY-0120 & Assembly de la courroie de l'axe Y & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Collier nylon 200mm & 2 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/AXY/DSC02383.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/AXY/DSC02384.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Prendre deux colliers nylon et faire un anneau du premier et passer l'autre dans l'anneau et dans la courroie pour faire la jonction. Passer l'anneau dans l'autre Screws M3x20mm à tête fraisée du support plateau et tendre la courroie en resserrant le collier. & Attention au sens de Assembly (voir photos). Ne pas trop tendre la courroie, le support plateau doit pouvoir se déplacer sans forcer.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%AXY-0130
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
AXY-0130 & Assembly des ressorts sur le plateau chauffant & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 16/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
RONDELLE\_PLATEAU & 4 & printed parts\\
\hline
Ressort & 4 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/AXY/DSC02539.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/AXY/DSC02540.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Placer les ressorts sur les Screws M3x40mm puis les RONDELLE\_PLATEAU à l'envers (le diamètre le plus petit doit rentrer dans les ressorts). & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%AXY-0140
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
AXY-0140 & Assembly du contact de fin de course Y & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 16/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
CLIP\_ENDSTOP\_Y & 1 & printed part\\
\hline
Screws M3x25mm & 2 & \\
\hline
Rondelles M3 standards & 4 & \\
\hline
Standard M3 nuts & 2 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/AXY/DSC02544.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter le CLIP\_ENDSTOP\_Y avec les Screws M3x25mm pour bloquer le contact de fin de course Y. Laisser dépasser le contact de fin de course jusqu'à apercevoir ses trous de fixation. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%AXY-0150
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
AXY-0150 & Assembly du plateau chauffant & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 16/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
MOLETTE\_GRANDE & 4 & printed parts, avec les écrous Nylstop\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/AXY/DSC02545.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter le plateau chauffant sur le support plateau en bois. Serrer les molettes pour avoir environ 2mm de Screws dépassant sous l'écrou. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%Section CHX : Assembly du chariot X
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\section{CHX - Assembly du chariot X}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CHX-0010
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CHX-0010 & Assembly pignon laiton sur moteur & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Moteur NEMA17 & 1 & \\
\hline
Pignon laiton & 1 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/CHX/DSC02327.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter le pignon laiton sur l'arbre moteur à environ 3-4 mm du boitier moteur. Serrer la Screws BTR avec une clé adaptée.  & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CHX-0020
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CHX-0020 & DéScrewssage des Screws du moteur de l'extrudeur & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Moteur NEMA17 & 1 & le même qui vient de recevoir le pignon laiton\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/CHX/DSC02328.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Enlever les deux Screws du côté de la fiche de connexion du moteur. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CHX-0030
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CHX-0030 & Assembly du support roulement sur l'extrudeur & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
EXTRUDEUR & 1 & printed part\\
\hline
EXTRUDEUR\_SUPPORT\_608ZZ & 1 & printed part\\
\hline
Screws M3x40mm à tête fraisée & 1 & \\
\hline
Rondelle M3 standard & 1 & \\
\hline
Ecrou M3 Nylstop & 1 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CHX/DSC02329.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CHX/DSC02330.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter l'EXTRUDEUR\_SUPPORT\_608ZZ sur l'EXTRUDEUR avec la Screws M3x40mm à tête fraisée et l'écrou Nylstop. Ne pas oublier la rondelle.  & Gratter l'intérieur de la charnière s'il y a des bavures.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CHX-0040
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CHX-0040 & Assembly du moteur sur l'extrudeur + roulement 608ZZ & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Screws M3x40mm & 2 & \\
\hline
Rondelles M3 standards & 2 & \\
\hline
Roulement 608ZZ & 1 & \\
\hline
Tige M8x25mm & 1 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/CHX/DSC02331.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter le moteur sur l'extrudeur avec les Screws M3x40mm dans les trous dont les Screws ont été enlevées. Ajouter le roulement et sa tige M8x25mm.  & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CHX-0050
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CHX-0050 & Assembly des molettes sur ressort de l'extrudeur & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
MOLETTE\_PETITE & 2 & avec Screws M3x60mm montées\\
\hline
Ressort & 2 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/CHX/DSC02332.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Screwsser les molettes en ajoutant les ressorts de compression sur l'extrudeur. Ne pas trop les serrer pour le moment (voir photo).  & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CHX-0060
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CHX-0060 & Assembly des supports de douilles sur le chariot X & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
FIX\_CHARIOT\_X\_1LM8UU & 1 & \\
\hline
FIX\_CHARIOT\_X\_2LM8UU & 1 & \\
\hline
Screws M3x8mm & 4 & \\
\hline
Rondelles M3 standards & 4 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/CHX/DSC02334.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Screwsser les deux printed parts sur la plaque en laissant la FIX\_CHARIOT\_X\_1LM8UU ouverte pour le moment. & Attention au sens, les trous fraisés de la plaque aluminium doivent être vers le haut.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CHX-0070
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CHX-0070 & Ajout de la tête d'impression sur le chariot X & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Tête d'impression & 1 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/CHX/DSC02335.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Ajouter la tête d'impression dans la découpe et finir de monter la printed part FIX\_CHARIOT\_X\_1LM8UU. & Faire sortir les fils de la tête d'impression du côté droite de la plaque aluminium.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CHX-0080
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CHX-0080 & Fixation des douilles linéaires sur le chariot X & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Douilles à billes linéaires LM8UU & 3 & \\
\hline
Colliers de serrage 200mm & 6 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/CHX/DSC02336.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Serrer les douilles à billes avec les colliers de serrage. & Bien faire attention au sens de Assembly des colliers (voir photo).\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CHX-0090
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CHX-0090 & Ajout des Screws de fixation de la courroie sur le chariot X & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Screws M3x20mm à tête fraisée & 2 & \\
\hline
Rondelles M3 standards & 2 & \\
\hline
Nylstop M3 nuts & 2 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CHX/DSC02338.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CHX/DSC02339.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Après avoir coupé les colliers nylon, monter les Screws M3x20mm à tête fraisée dans les trous prévus à cet effet. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CHX-0100
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CHX-0100 & Fixation de l'extrudeur le chariot X & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Screws M3x20mm & 2 & \\
\hline
Rondelles M3 standards & 2 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/CHX/DSC02340.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter l'extrudeur avec les Screws M3x20mm. Ne pas oublier les rondelles sous la plaque aluminium. & Le serrage de l'extrudeur permet de bloquer la tête d'impression. S'assurer qu'elle est bien en butée avant de serrer.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%Section AXX : Assembly de l'axe X
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\section{AXX - Assembly de l'axe X}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%AXX-0010
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
AXX-0010 & Assembly des écrous M5 dans les SUPPORT\_AXE\_X & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
SUPPORT\_AXE\_X & 2 & \\
\hline
Screws agglo 4x20mm tête bombée & 4 & \\
\hline
Rondelles M4 standards & 4 & \\
\hline
Ecrous M5 & 2 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/AXX/DSC02341.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Insérer les écrous M5 et les maintenir en Screwssant les Screws avec les rondelles. & Vérifier l'alignement de l'écrou avec une tige filetée M5.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%AXX-0020
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
AXX-0020 & Assembly de l'axe Y & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
SUPPORT\_AXE\_X & 2 & \\
\hline
SUPPORT\_ENDSTOP\_X & 1 & \\
\hline
Arbre de guidage 8x315mm & 2 & \\
\hline
Chariot X & 1 & \\
\hline
Screws M3x20mm & 5 & \\
\hline
Rondelles M3 standards & 5 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.8\textwidth]{images/AXX/DSC02342.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter les arbres de guidage dans les SUPPORT\_AXE\_X sans oublier le SUPPORT\_ENDSTOP\_X (à gauche) et le chariot X. L'entraxe entre les deux SUPPORT\_AXE\_X doit être de \textbf{287.5mm (flèche double)}. Attention au sens de Assembly, le SUPPORT\_AXE\_X avec l'écrou Nylstop (flèche rouge à gauche) doit être monté à gauche. Serrer ensuite les Screws M3x20mm avec leur rondelle (points verts sur la photo). & Utiliser un petit marteau ou maillet en caoutchouc pour enfoncer les arbres sans trop forcer pour éviter d'endommager les printed parts. Si cela force trop, repercer les pièces avec un forêt de 8mm. Ne pas trop serrer les Screws pour éviter d'endommager les printed parts. Mettre un point de superglue sur les écrous pour bloquer le Assembly.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%AXX-0030
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
AXX-0030 & Assembly poulie aluminium sur moteur & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Moteur NEMA17 & 1 & \\
\hline
Poulie aluminium & 1 & \\
\hline
Screws M3x8mm & 1 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/AXX/DSC02343.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter la poulie aluminium sur l'arbre moteur en laissant environ 2mm entre la poulie et le bloc moteur. Serrer avec la Screws M3x8mm. & Serrer la Screws sur le méplat de l'arbre moteur.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%AXX-0040
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
AXX-0040 & Assembly moteur sur l'axe X & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Moteur NEMA17 & 1 & précédemment monté avec la poulie aluminium\\
\hline
Screws M3x25mm & 2 & \\
\hline
Rondelles M3 standards & 2 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/AXX/DSC02344.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/AXX/DSC02345.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Screwsser le moteur sur le SUPPORT\_AXE\_X de gauche avec les Screws M3x25mm et leur rondelle. & Faire attention à l'orientation du connecteur du moteur (voir photo).\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%AXX-0050
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
AXX-0050 & Assembly du RETOUR\_X & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
RETOUR\_X & 2 & printed parts\\
\hline
Roulement 608ZZ & 1 & \\
\hline
Screws M3x30mm & 3 & \\
\hline
Rondelles M3 standards & 6 & \\
\hline
Standard M3 nuts & 3 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/AXX/DSC02346.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter le roulement 608ZZ en sandwich entre les RETOUR\_X et serrer avec les Screws M3x30mm et leurs rondelles. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%AXX-0060
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
AXX-0060 & Assembly de la courroie de l'axe X & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Courroie 680mm & 1 & \\
\hline
Collier nylon 200mm & 1 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/AXX/DSC02347.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Faire une boucle avec la courroie et la bloquer en serrant bien le collier nylon. Fixer la courroie sur la Screws M3x20mm à tête fraisée du chariot X et la passer autour de la poulie. & Finir de serrer le collier nylon autour de la Screws pour qu'il n'y ai pas de jeu autour de la boucle.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%AXX-0070
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
AXX-0070 & Assembly de la courroie de l'axe X & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
 &  & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/AXX/DSC02348.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Faire faire un demi tour à la courrie afin que le plat soit en contact avec le roulement 608ZZ. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%AXX-0080
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
AXX-0080 & Assembly de la courroie de l'axe X & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Collier nylon 200mm & 1 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/AXX/DSC02349.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Faire une boucle très serrée à l'autre extrémité de la courroie avec un collier nylon de 200mm. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%AXX-0090
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
AXX-0090 & Assembly de la courroie de l'axe X & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 13/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Collier nylon 200mm & 2 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/AXX/DSC02350.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/AXX/DSC02352.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Prendre deux colliers nylon et faire un anneau du premier et passer l'autre dans l'anneau et dans la courroie pour faire la jonction. Passer l'anneau dans l'autre Screws M3x20mm à tête fraisée du chariot X et tendre la courroie en resserrant le collier. & Attention au sens de Assembly (voir photos). Ne pas trop tendre la courroie, le chariot Y doit pouvoir se déplacer sans forcer.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%Section POR : Assemblage du portique
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\section{POR - Assemblage du portique}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%POR-0010
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
POR-0010 & Assembly des FIXATION\_PORTIQUE sur les tubes & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
FIXATION\_PORTIQUE & 3 & printed parts\\
\hline
FIXATION\_PORTIQUE\_ENDSTOP\_Z & 1 & printed part\\
\hline
Tubes 12x415mm & 4 & \\
\hline
Screws M3x10mm & 4 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/POR/DSC02387.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/POR/DSC02388.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter un tube dans la BASE\_Z dans le châssis et bloquer la FIXATION\_PORTIQUE pour que le haut de la printed part affleure le bois. Monter les trois autres pièces de la même manière et les bloquer avec les Screws M3x10mm sans trop serrer pour ne pas endommager les pièces. La hauteur indicative est de 75mm (double flèche rouge). & Attention au sens de Assembly (voir photos). Les Screws de blocages doivent se retrouver à l'extérieur des futurs portiques.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%POR-0020
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
POR-0020 & Remplacement des Screws sur les moteurs NEMA14 & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Moteur NEMA14 & 2 & \\
\hline
Screws M3x40mm & 8 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/POR/DSC02390.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
DéScrewsser les Screws des blocs des moteurs NEMA14 et les remplacer par les Screws M3x40mm. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%POR-0030
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
POR-0030 & Fixation des moteurs NEMA14 & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
FIX\_MOTEUR\_Z & 2 & printed parts \\
\hline
Moteur NEMA14 & 2 & avec Screws remplacées \\
\hline
Rondelles M3 standards & 8 & \\
\hline
Standard M3 nuts & 8 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/POR/DSC02392.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter les moteurs sur les FIX\_MOTEUR\_Z et bien serrer le Assembly. & Attention au sens de Assembly des câbles des moteurs (voir photo).\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%POR-0040
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
POR-0040 & Assembly côté gauche du portique & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Screws M3x10mm & 2 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/POR/DSC02393.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter le portique de gauche et verrouiller avec les Screws M3x10mm sur la pièce FIXATION\_MOTEUR\_Z. La hauteur entre le bout du tube et le bas de la pièce est de 33mm (double flèche rouge). & Attention au sens de Assembly des tubes et du placement des Screws de blocage (voir photo, la pièce FIXATION\_PORTIQUE\_ENDSTOP\_Z est en bas).\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%POR-0050
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
POR-0050 & Assembly côté droit du portique & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 18/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Screws M3x10mm & 2 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/POR/DSC02395.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter le portique de droite et verrouiller avec les Screws M3x10mm sur la pièce FIXATION\_MOTEUR\_Z. La hauteur entre le bout du tube et le bas de la pièce est de 33mm (double flèche rouge). & Attention au sens de Assembly des tubes et du placement des Screws de blocage (voir photo).\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%POR-0060
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
POR-0060 & Assembly des tiges filetées & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Tiges filetées M5x345mm & 2 &  \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/POR/DSC02398.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter les COUPLAGE\_Z et les tiges filetées sur les arbres moteurs. Ne pas serrer pour l'instant. & Si les arbres moteurs ou les tiges filetées ont du mal à rentrer, il est possible de taper doucement sur les éléments avec un marteau.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%POR-0070
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
POR-0070 & Ebavurage des SUPPORT\_AXE\_X & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Palier linéaire 12mm & 1 &  \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/POR/DSC02400.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Ebavurer les SUPPORT\_AXE\_X pour que les paliers de 12mm puissent se mettre sans forcer. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%POR-0080
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
POR-0080 & Assemblage du portique gauche & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Palier linéaire 12mm & 2 &  \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/POR/DSC02401.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Placer deux paliers linéaires sur les tubes et commencer à Screwsser la tige filetée du portique de gauche dans l'axe X. & Attention au sens, le portique de gauche est celui ayant le support pour le contact de fin de course Z (flèche rouge en bas).\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%POR-0090
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
POR-0090 & Assemblage du portique droite & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Palier linéaire 12mm & 2 &  \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/POR/DSC02402.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Répéter l'opération pour le portique droit. & Ne pas oublier les paliers linéaires de 12mm.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%POR-0100
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
POR-0100 & Ajout des TOP\_Z sur le portique & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
TOP\_Z & 2 & printed parts \\
\hline
Palier linéaire 12mm & 4 &  \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/POR/DSC02408.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Ajouter les 4 derniers paliers 12mm puis monter les TOP\_Z et les serrer. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%POR-0110
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
POR-0110 & Serrage des accouplements & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
 &  &  \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/POR/DSC02405.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Maintenant que les portiques sont complets, serrer les accouplements pour les bloquer (sans forcer pour ne pas endommager les pièces). & Faire tourner les tiges filetées pendant le serrage pour s'assurer de ne pas avoir de désaxement.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%POR-0120
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
POR-0120 & Assembly du portique dans le châssis & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
 &  &  \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/POR/DSC02410.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/POR/DSC02409.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Positionner le portique dans le châssis en l'enfonçant dans les BASE\_Z. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%POR-0130
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
POR-0130 & Blocage du portique & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
MOLETTE\_GRANDE & 4 & printed parts, avec Screws M3x30mm \\
\hline
Rondelles M3 larges & 20 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/POR/DSC02411.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/POR/DSC02412.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Mettre 5 rondelles par molette et serrer dans les trous sur le côté du châssis pour bloquer le portique. Répéter l'opération pour les 4 molettes. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%POR-0140
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
POR-0140 & Collage des paliers & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
 &  &  \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/POR/DSC02413.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Coller les 8 paliers avec de la superglue (de préférence en gel). & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%POR-0150
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
POR-0150 & Assembly de la Screws de réglage de l'offset Z & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
MOLETTE\_GRANDE & 1 & avec Screws M3x40mm \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/POR/DSC02414.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Screwsser la molette de réglage au niveau de l'écrou Nylstop dans le SUPPORT\_AXE\_X de gauche. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%Section CAB : Câblage
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\section{CAB - Câblage}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CAB-0005
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Tableau titre et description
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{N° fiche} & \textbf{Description} & \textbf{Type}\\
\hline
CAB-0005 & Schéma de branchement sur la carte & Schéma\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Tableau de gestion des versions
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Révision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 24/01/2014 & Première version de la fiche & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.8\textwidth]{images/CAB/DSC01000.JPG}
\vspace{0.5cm}

\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CAB-0007
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Tableau titre et description
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{N° fiche} & \textbf{Description} & \textbf{Type}\\
\hline
CAB-0007 & Branchement du plateau chauffant & Câblage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Tableau de gestion des versions
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Révision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 24/01/2014 & Première version de la fiche & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Nomenclature des pièces
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Désignation} & \textbf{Quantité} & \textbf{Notes}\\
\hline
 &  &  \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=1\textwidth]{images/CAB/DSC02582.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Astuces, conseils}\\
\hline
Brancher les connecteurs du plateau chauffant. De haut en bas : résistances plateau, contact fin de course Y et thermistance (contact 2 pôles de gauche). & Il n'y a pas de polarité pour les résistances, connecter les deux fils sur les bornes les plus éloignées du bornier.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CAB-0010
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CAB-0010 & Assembly du contact de fin de course Z & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Contact de fin de course & 1 & avec 500mm de câble \\
\hline
Screws M3x20mm & 1 &  \\
\hline
Rondelle M3 standard & 1 &  \\
\hline
Ecrou M3 standard & 1 &  \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02424.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02426.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter le contact de fin de course et le pincer avec la Screws M3x20mm et l'écrou. Brancher ensuite le connecteur Molex sur la carte électronique. & Attention au sens de Assembly, la partie charnière du contact est à droite.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CAB-0020
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CAB-0020 & Assembly du contact de fin de course X & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Contact de fin de course & 1 & avec 900mm de câble \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02425.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02427.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter le contact de fin de course par collage avec de la superglue. Utiliser une presse ou pince à linge pour le maintenir durant le séchage. Brancher ensuite le connecteur Molex sur la carte électronique. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CAB-0030
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CAB-0030 & Câblage du moteur Y & Câblage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Câble moteur 200mm & 1 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02429.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02430.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Brancher le câble de 200mm au moteur de l'axe Y et brancher ensuite le connecteur Molex sur la carte. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CAB-0040
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CAB-0040 & Câblage du moteur X & Câblage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Câble moteur 900mm & 1 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02432.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02433.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Brancher le câble de 900mm au moteur de l'axe X et brancher ensuite le connecteur Molex sur la carte. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CAB-0050
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CAB-0050 & Câblage des moteurs Z & Câblage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
 &  & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02435.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02436.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Passer les câbles des moteurs Z sous les arbres de guidage. Couper le câble du moteur Z de droite à environ 35cm et démonter le connecteur Molex du moteur de gauche. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CAB-0060
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CAB-0060 & Câblage des moteurs Z & Câblage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
 &  & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02437.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02438.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Souder les fils du câble du moteur de droite sur les fiches du moteur de gauche et remonter le connecteur Molex. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CAB-0070
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CAB-0070 & Câblage des moteurs Z & Câblage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
 &  & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/CAB/DSC02439.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Brancher le connecteur Molex des moteurs Z sur la carte. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CAB-0080
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CAB-0080 & Câblage du moteur E & Câblage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Câble moteur 1300mm & 1 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02434.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02440.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Brancher le câble de 1300mm au moteur de l'axe X et brancher ensuite le connecteur Molex sur la carte. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CAB-0090
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CAB-0090 & Câblage ventilateur de boitier électronique & Câblage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
 &  & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/CAB/DSC02441.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Brancher le connecteur Molex du ventilateur de boitier sur la carte, peut importe le sens, il faudra voir en mettant l'imprimante sous tension si le branchement est correct et si le ventilateur tourne. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CAB-0100
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CAB-0100 & Rallonge câbles tête d'impression & Câblage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Paire RJ45 300mm & 1 & \\
\hline
Câble double $0.75mm²$ 300mm & 1 & \\
\hline
Gaîne thermorétractable & 1 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02444.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02445.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Si les câbles de la tête d'impression ne font pas 1300mm, les rallonger avec du fil et protéger les soudures avec de la gaîne thermorétractable. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CAB-0110
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CAB-0110 & Soudure connecteur Molex thermistance tête d'impression & Câblage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Contacts Molex & 2 & \\
\hline
Connecteur Molex 2 pôles & 1 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02446.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02447.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Souder les fiches Molex sur les fils de la thermistance et monter le connecteur Molex. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CAB-0120
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CAB-0120 & Branchement tête d'impression & Câblage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
 &  & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/CAB/DSC02448.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Brancher le connecteur de la thermistance (en bas) et Screwsser les fils de la résistance de chauffe en haut. & Les branchements n'ont pas de polarité, ils peuvent être inversés. Dans le cas où il y aurait 4 fils pour la résistance, les brancher par groupe de deux (1 paire pour le ++ et une paire pour le - -).\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CAB-0130
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CAB-0130 & Branchement alimentation 12V & Câblage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
 &  & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/CAB/DSC02449.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Brancher les fils 12V provenant de l'alimentation électrique sur le bornier de la carte. & Il est plus facile d'insérer les fils en les étamant au préalable. Attention au sens de Assembly (le plus est à droite).\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CAB-0140
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CAB-0140 & Installation LED & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
SUPPORT\_FAN\_X & 1 & printed part\\
\hline
LED précâblée & 1 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02463.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02464.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Enlever l'écrou et la rondelle de la LED puis la Screwsser dans le SUPPORT\_FAN\_X. & Ebavurer le trou et mettre un point de superglue pour bien bloquer la LED si nécessaire. \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CAB-0150
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CAB-0150 & Assembly ventilateur X & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Ventilateur 40mm & 1 & \\
\hline
Screws M3x20mm & 2 & \\
\hline
Rondelles M3 standards & 2 & \\
\hline
Nylstop M3 nuts & 2 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02465.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02467.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Screwsser le ventilateur sur le SUPPORT\_FAN\_X. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CAB-0160
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CAB-0160 & Rallonge des câbles X & Câblage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Paire RJ45 1300mm & 2 & \\
\hline
Gaîne thermorétractable &  & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02479.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02472.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Rallonger les câbles pour atteindre les 1300mm pour ensuite mettre des connecteurs Molex 2 pôles au bout. & Attention à la polarité pour le ventilateur, le +V est le 12V et le 0 le 0V (voir photo). Pour la LED, le 0V est le câble noir. Pour bien repérer les câbles, mettre le 0V avec le fil RJ45 le plus clair.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CAB-0170
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CAB-0170 & Assembly du ventilateur & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Screws M3x60mm & 1 & \\
\hline
Rondelle M3 standard & 2 & \\
\hline
Ecrou M3 Nylstop & 1 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/CAB/DSC02473.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter le bloc sur le chariot X avec la Screws M3x60mm et l'écrou Nylstop en bout. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CAB-0180
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CAB-0180 & Branchement sur la carte & Câblage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
 &  & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/CAB/DSC02474.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Passer les câbles dans le châssis et les brancher sur les pins 12V disponibles de la carte électronique. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CAB-0190
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CAB-0190 & Assembly interrupteur en façade & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Interrupteur rond & 1 & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/CAB/DSC02476.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Monter l'interrupteur en façade dans le trou prévu à cet effet. & La Screws de blocage ne peut être mise à cause de l'épaisseur du bois.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%CAB-0200
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
CAB-0200 & Câblage interrupteur de façade & Câblage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
 &  & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02477.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/CAB/DSC02478.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Prendre un fil du ventilateur du chariot X et le couper pour ensuite le souder sur l'interrupteur. Mettre un point de superglue dans le bois une fois fini pour bloquer l'interrupteur. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%Section TFW : Téléversement du firmware
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\section{Téléversement du firmware}
\newpage
Le firmware est le microprogramme installé dans la puce ATMega de la carte Sanguinololu. Il permet de contrôler l'imprimante, de définir si les moteurs doivent tourner dans tel ou tel sens, de remonter les infos des capteurs...\\

Cette documentation a été rédigée en faisant les essais sous Windows. Les étapes sont similaires sur les autres systèmes.
\subsection{Installation des drivers de la carte électronique}
Brancher le câble USB de votre Tobeca\textregistered~ sur votre ordinateur. Les drivers devraient s'installer automatiquement. Si ce n'est pas le cas (erreur type \textbf{le driver n'a pas pu être installé}), installer manuellement les drivers depuis le CD, présent dans le dossier \textbf{Drivers}.
\subsection{Récupération de l'IDE Arduino}
L'IDE Arduino est un interpréteur de code. Il va permettre de téléverser le firmware pour la Tobeca\textregistered~, directement dans la puce ATMega de la Sanguinololu.\\

L'archive est disponible pour chaque architecture (Windows, Mac, Linux) sur le CD, dans le dossier \textbf{Softwares}. Elle est complète et déjà préparée pour fonctionner avec la carte Sanguinololu.\\

Décompresser le dossier de l'IDE dans le répertoire de votre choix.
\subsection{Configuration du firmware pour la Tobeca\textregistered~}
Les sources du firmware sont disponibles sur le CD, dans le dossier \textbf{Sources/FW}.\\

Charger le fichier \textbf{Marlin.pde} avec l'IDE Arduino précédemment décompressé, qui ouvrira tous les fichiers correspondants au firmware.\\

Le firmware intègre plusieurs réglages en fonction des versions de la Tobeca\textregistered~. Ceux ci sont dans le fichier \textbf{configuration.h}, aux environs de la ligne 111 pour les réglages de thermistance et 282 pour les réglages de pas.
\subsection{Réglage de la thermistance}
En fonction de la tête d'impression qui est montée sur la Tobeca\textregistered~, il peut être nécessaire de modifier la valeur de la thermistance :\\

\begin{tt}
\small{
\#define TEMP\_SENSOR\_0 5\\
}
\end{tt}

De base le réglage est sur la thermistance n°5 pour une J-Head. Si cependant après un flashage de la carte la valeur mesurée par la thermistance est aberrante, réessayer en passant la valeur à \textbf{1} ou \textbf{11} et reflasher le firmware.
\subsection{Réglage des pas / mm}
\begin{tt}
\small{
//\#define DEFAULT\_AXIS\_STEP\_PER\_UNIT   {46, 46, 2560,152}    // from TO-003 to TO-006 (T5)\\
//\#define DEFAULT\_AXIS\_STEPS\_PER\_UNIT   {46, 64, 2560,152}    // from TO-007 to TO-015 (T5)\\
//\#define DEFAULT\_AXIS\_STEPS\_PER\_UNIT   {64, 64, 2560,152}    // from TO-016 to TO-045 (T5)\\
//\#define DEFAULT\_AXIS\_STEPS\_PER\_UNIT   {64, 64, 4000,152}    // from TO-046 to TO-048 (T5 + M5)
\#define DEFAULT\_AXIS\_STEPS\_PER\_UNIT   {66.67, 66.67, 4000,152}    // from T0-049 to TO-0 (HTD3M + M5)
}
\end{tt}

En fonction du n° de série de votre Tobeca\textregistered~, il faut décommenter la bonne ligne, car les réglages des pas / mm diffèrent en fonction des modèles de poulies fournies. Pour décommenter une ligne, il faut enlever les / devant.\\

Une seule ligne doit être décommentée, sinon la compilation du firmware ne fonctionnera pas.

\subsection{Téléversement du firmware}
\begin{itemize}
\item Brancher la carte Sanguinololu en USB au PC.\\
\item Lancer l'IDE Arduino (aller dans le dossier d'installation et lancer \textbf{arduino.exe}).\\
\item Ouvrir un nouveau projet (File $\rightarrow$ Open) et choisir le fichier \textbf{marlin.pde} dans le dossier du firmware pour la Tobeca\textregistered~.\\
\item Aller dans l'onglet Tools $\rightarrow$ Board et choisir la carte \textbf{Sanguino W/ATmega 1284p 16mhz}.\\
\item Aller dans l'onglet Tools $\rightarrow$ Port et choisir le port COM de la carte Sanguinololu (normalement il n'y a qu'un seul port à choisir).\\
\item Cliquer ensuite sur le bouton \textbf{Upload} (passer au dessus des boutons pour voir leur description).\\
\item Le firmware va se compiler et se téléverser sur la carte. Un message indique la fin du téléversement.
\end{itemize}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%Section PMR : Première mise en route
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\section{Première mise en route}
\newpage

Après avoir téléversé le firmware pour la carte électronique, il faut valider la bonne marche des fonctions de la Tobeca\textregistered~.\\

Utiliser pour cela Repetier Host pour se connecter à l'imprimante (voir guide d'utilisation de la Tobeca\textregistered~) et tester les points suivants :\\

\begin{itemize}
\item Déplacement des axes X, Y et Z
\item Bon fonctionnement des fins de course X, Y et Z
\item Chauffe de la tête d'impression
\item Rotation du moteur d'extrudeur quand la tête est à plus de 190°C.
\item Chauffe du plateau chauffant\\
\end{itemize}

Si tout est OK, alors les finitions peuvent être réalisées.\\

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%Section FIN : Finitions
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\section{FIN - Finitions}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%FIN-0010
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
FIN-0010 & Assembly du support de bobines & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
SUP\_BOBINE\_BAS & 1 & printed part \\
\hline
SUP\_BOBINE\_HAUT & 1 & printed part \\
\hline
Screws M8x100mm & 1 &  \\
\hline
Roulements 608ZZ & 2 &  \\
\hline
Ecrou M8 & 1 &  \\
\hline
Ecrou M8 papillon & 1 &  \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.4\textwidth]{images/FIN/DSC02451.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.4\textwidth]{images/FIN/DSC02452.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Positionner les roulements 608ZZ dans les printed parts. Ebavurer les trous si nécessaire. & Utiliser la Screws M8x100mm avec un écrou pour mettre en place les roulements dans les pièces en frappant avec un marteau.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%FIN-0020
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
FIN-0020 & Assembly du support de bobines & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
 &  &  \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/FIN/DSC02453.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Mettre en place le support de bobines sur un des TOP\_Z. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%FIN-0030
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
FIN-0030 & Mise en place de la spirale de câble & Câblage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Spirale de câble & 1.5m &  \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/FIN/DSC02480.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/FIN/DSC02481.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Commencer à mettre la spirale à partir du chariot X. & Mettre le chariot X en butée à droite pour bien voir la longueur de fil nécessaire pour les déplacements.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%FIN-0040
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
FIN-0040 & Mise en place de la spirale de câble & Câblage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Collier nylon 200mm & 2 &  \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/FIN/DSC02482.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Rassembler les câbles au niveau du SUPPORT\_AXE\_X de gauche et maintenir la spirale avec deux colliers nylon. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%FIN-0050
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
FIN-0050 & Mise en place de la spirale de câble & Câblage\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
Collier nylon 200mm & 2 &  \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/FIN/DSC02508.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Bloquer la spirale en bas du portique de gauche avec deux colliers nylon de 200mm, directement sur les tubes des portiques. & Mettre l'axe X en position assez haute pour bien voir la longueur de câble nécessaire pour l'élévation en Z.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%FIN-0060
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
FIN-0060 & Mise en place de la spirale de câble & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
 &  &  \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=\textwidth]{images/FIN/DSC02483.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|c|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Regrouper les câbles avec la spirale jusque dans le boitier électronique. & \\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%FIN-0070
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\begin{center}
%Title and description table
\begin{tabularx}{\textwidth}{|c|X|c|}
\hline
\textbf{Form n°} & \textbf{Description} & \textbf{Type}\\
\hline
FIN-0070 & Mise en place de la spirale de câble & Assembly\\
\hline
\end{tabularx}
\vspace{0.5cm}

%Changelog table
\begin{tabularx}{\textwidth}{|c|c|X|c|}
\hline
\textbf{Revision} & \textbf{Date} & \textbf{Description} & \textbf{Notes}\\
\hline
AA & 14/01/2014 & First version of the form & \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Parts list
\begin{tabularx}{\textwidth}{|c|c|X|}
\hline
\textbf{Description} & \textbf{Quantity} & \textbf{Notes}\\
\hline
SANGUINOLOLU\_TOP &  & printed part \\
\hline
Colliers nylon 100mm &  & en fonction du besoin \\
\hline
\end{tabularx}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/FIN/DSC02484.JPG}
\vspace{0.5cm}

%Image
\includegraphics[width=0.5\textwidth]{images/FIN/DSC02485.JPG}
\vspace{0.5cm}

%Instructions
\begin{tabularx}{\textwidth}{|X|X|}
\hline
\textbf{Instructions} & \textbf{Tips, warnings}\\
\hline
Regrouper les câbles du moteur Z de gauche. Ranger les câbles dans le boitier et fermer avec le capot. & Si nécessaire, regrouper des câbles à l'intérieur du boitier avec des colliers nylon de 100mm.\\
\hline
\end{tabularx}
\end{center}

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
%Section RCT : Réglages finaux, calibration et tests
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\newpage
\logotobeca
\section{Réglages finaux}
\newpage
\subsection{Vérification de la tension des courroies}
Pour les impressions soient réussies, il faut que les courroies soient assez tendues mais pas trop. Si elles sont trop tendues, les moteurs n'auront pas assez de puissance pour les entraîner. Si par contre elles ne sont pas assez tendues, les déplacements créeront des phénomènes de jeux d'entre-dent, ce qui se manifestera pas un mauvais positionnement de la tête et donc réduira la qualité des impressions.
\subsection{Préparation et calibration du plateau d'impression}
La procédure de calibration du plateau d'impression est disponible dans le Guide d'utilisation de la Tobeca\textregistered~. La procédure ne change pas entre une imprimante neuve et un réglage de routine.
\subsection{Réglage de la puissance des drivers de moteurs pas à pas}
Avant de tester votre première impression, il faut vérifier la puissance des drivers de moteurs en ajustant le potentiomètre de chaque driver sur la carte électronique :

\begin{center}
%Image
\includegraphics[width=\textwidth]{images/REGLAGES_FINAUX/DSC02460.JPG}
\vspace{0.5cm}
\end{center}
Augmenter la puissance augmente le sifflement entendu au niveau des moteurs. Il faut ne pas trop augmenter la puissance car les drivers vont chauffer et peuvent se mettre en sécurité, ce qui peut bloquer le moteur pendant quelques secondes et donc faire rater des impressions.

Le plus simple est donc de tester des impressions et voir si les moteurs se déplacent bien à vitesse élevée (déplacements sans impression).

Une fois vos tests faits, votre Tobeca\textregistered~ est terminée !


\end{document}